Configuration LAN (Fibroscan directly on laptop)

PC Configuation :


-Click on Start

-Select « Control panel » and display by catégory


-Click on « display network statue »




-Click on local network connexion




-Click on Properties




-Doble Click on internet protocole version 4 (TCP/IPV4)




-fill as below and click on OK




-Create folder named « Fibroscan » to C :




-Right click on folder created and select properties




-Click on tab « Share » then click “to share”




-Select PC User, then click on “shared”




-Click on finish




-Click on advanced share



-Click on « autorisations »



-Select « All », check « Three boxs » and click on « Apply»



**ECHOSENS**

5 RUE JEAN LEMOINE

94000 CRETEIL – France

T: +33 1 49 81 89 29

M : [service@echosens.com](mailto:service@echosens.com)

[WWW.ECHOSENS.COM](http://www.echosens.com/)