CONFIDENTIEL

1. REQUIRED

Concerning this procedure, do you need those element :

- 402/430/530 (with or without probe)

- Electrical cordon

- A Echosens Software Flash Key

2. FIRST START UP

Insert the USB flash key at this moment. Start up your device normally

The device will start the restoring automatically (some black background and blue backround will appears) depending on the device it might reboot itself or just shut down, remove the USB thumbdrive and power on the device

If you have any question about this instruction, please join us at [service@echosens.com](mailto:service@echosens.com)

FibrosCan 430

­­­­­­­­­­­­­­-\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_-

1. REQUERIDO  
     
   En relación con este procedimiento, necesita estos elementos:  
     
   - 402/430/530 (con o sin sonda)  
     
   - Cordón eléctrico  
     
   - Una clave flash de Echosens Software  
     
   2. PRIMER ARRANQUE  
     
   Inserta la llave USB flash en este momento.

Enciende tu dispositivo normalmente.  
El dispositivo iniciará la restauración automáticamente (aparecerá un fondo negro y un fondo azul), dependiendo del dispositivo, podría reiniciarse o simplemente apagarse, quitar la unidad USB y encender el dispositivo.

Si tiene alguna pregunta sobre esta instrucción, únase a nosotros en [service@echosens.com](mailto:service@echosens.com)

FibrosCan 430