

Collimator board layout