Here are the current PACS setting on Springfield PACS server for Lithotripsy

Store Service Class Provider (SCP)

 Server name:- Springfield

Server AETitle:- sprirpfs01FIR

IP address 10.216.88.106

Port:- 2104

Worklist (SCP)

 Server name: Worklist

AETitle:- Kodak-XIS

IP address:- 10.216.152.17

Port:- 3320

The scanner ip details are the following:-

IP:- 10.216.88.122

S\N:- 255.255.252.0

G\W:- 10.216.88.1

AETitle:- SONOLITHISYS

Port:- 104